Use the below commands to block and allow ICMP or IP traffic

1. Command to deny ICMP packets

**access-list 110 deny icmp any any**

1. Command to allow IP packets

**access-list 110 permit ip any any**

1. Command to allow ICMP packets with host address

**access-list 110 permit icmp host 10.10.1.1 any**

**access-list 110 permit icmp host 10.10.1.1 any echo-reply**

1. Command to allow ICMP packets with host and interface address

**access-list 110 permit icmp host 10.10.1.1 any echo**

**interface Ethernet1/0**

**ip address 10.10.1.2 255.255.255.0**

Based on the question you can use the commands

Run all these command in Global command mode or CLI